|  |  |  |
| --- | --- | --- |
| Sentex Infinity DI Telephone Entry System |  | **Sentex Infinity DI this is an Apartment Intercoms for more than a 100 units**The Sentex Infinity DI is engineered for exceptional performance and functionality, combining the convenience of telephone entry with the flexibility of access control. [Sentex Infinity Specs](http://www.allsecurityequipment.com/manuals/sentex-infinity-specs.pdf) [Sentex Infinity Manual](http://www.liftmaster.com/consumerweb/pdfdocs/infin.pdf) **SPECIFICATIONS:*** Directory Codes: 500
* Full Entry Codes with Names: 3000
* Full Entry Codes without Names: 16,000
* Event Buffer: 5800
* Power: 12VAC @ 3.4 amps peak, 13.5VDC @ 2.1 amps (without readers)
* Dimensions: Infinity L & DI Surface Mount 21"H x 16-7/16"W x 4-3/8"D
* Infinity L & DI Flush Mount 21-5/6"H x 16-3/4"W x 3-1/8"D
* Shipping Weight: = 32 lbs.
* **This Model Is Discontinued. Please call for possible replacement.**
 |

## Sentex Infinity DI Features

**UNIQUE FEATURES:**

* Paper directory insert for typed names

**STANDARD FEATURES:**

* Full duplex communications
* Long distance and PBX dialing
* Tone/pulse compatibility
* Variable code length
* Battery backup
* Burglar alarm shunt
* Anti-glare
* Stainless steel housing
* Expanded transaction buffer
* Programmed talk time
* Shared phone line capability
* Controlled & programmable system relays
* Internal modem
* Lightning protection
* Full controls
* SPSWin programming software
* Non-volatile memory
* Transaction monitoring
* Password protection
* Forced door alarms
* Automatic unlock schedules
* Dual ventilation fans
* Postal lock provisio